# Electric fan remove and install

Remove radiator

Remove the three nuts and bolts securing the fan to the condenser.

Remove the condenser mounting bolts and tie the condenser back

Remove plastic trim from behind left headlight assembly

Disconnect condenser fan wiring and lift fan out gap created by tying back condenser.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson