# Group 24 Automatic Transmission Service Bulletins

#### Bulletin number

#### Title

#### Description

#### Date of issue

24 02 83 (805) | Revised oil pan tightening torque | Reduced torque to 4.5 - 5.0 ft lbs. | April 1984
24 01 85 (1012) | 4 HP 22 missing spring | Change transmission if spring is determined missing | June 1985
24 02 85 (1027) | Checking ATF fluid level | New dipstick 24 11 1 207 767 since 2/85, earlier dipsticks too short, change with new one | July 1985
24 03 87 (1524) | ZF 4 HP 22 Service Action E30 2/86 to 4/86 | Poor quality A clutch , replace clutch | January 1988
24 05 89 (1945) | Transmission Oil Dipstick, revision | New handle on dipstick, tilt to release. | September 1989
24 06 89 (1963) | Automatic transmission pickup screen | Deeper filter to prevent suction noises | January 1990
24 03 90 (3109) | Correct adjustment of shift cable | Improper adjustment after repairs can result in poor shifting | September 1990

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson