# Window 2 door rear side glass trim replace

The frame surrounding the rear window is available in three separate pieces. Replacement of individual pieces requires the following :

Remove window

Pull frame from rubber seal.

Drill out rivets located in each corner of the frame.

Insert new section(s) of frame and install new rivets

Replace rubber seal if necessary.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson