# Accelerator pedal, replace

CAUTION: Never re-use an accelerator pedal, lower clips on pedal get damaged during removal and could cause the pedal to come loose while driving. Always install a new pedal if it is removed for any reason.
Remove circlip from upper pedal pivot and slide pedal off shaft on lever. |
Push down carpet behind pedal, squeeze and push out clips on lower end of pedal.

### Installation

Ensure that lower clips engage correctly.

### Part numbers

Accelerator pedal , up to 9/87 production : 35 41 1 118 210
Accelerator pedal , from 9/87 production : 35 41 1 156 488

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson