# Fuel filter, replace

Some models have the fuel filter located on the left frame rail , beside the steering column On most, it is located just forward of the left rear wheel on most models, actual position varies slightly on some models. |  |
Remove fuel pump fuse. (Fuse 11, see fuse allocation for location)
After engine stalls, turn off ignition
Remove clamps from fuel hoses and remove hoses. |  |
Remove 10mm bolt securing filter bracket to body, or loosen large clamps and slide filter out, depending on which style you have. |
Ensure filter is installed in the correct orientation. Filter has an arrow and should have the word OUT at the outlet end.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson