Power steering, fill and bleed

# Power steering, filling and bleeding system

Fill power steering fluid reservoir with standard Dexron III Automatic Transmission Fluid (ATF) to the MAX mark on the reservoir

Start engine, turn steering wheel to full lock in each direction twice.
Do not hold wheel against lock for an extended period of time.

Stop engine and check level, top off to MAX mark.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson